**Zebtec Maintenance Checklist**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Month** | **Check pH & Conductivity Probes for Damage****Monthly** | **Float Switches Water Level****Monthly** | **Drum Filter Washing Pressure Gauge =7 Bars****Monthly** | **Carbon Filter Replace if PSI >10****Monthly** | **Biofilter Air Distribution****Every 3 months** | **Check Sump Level****Every 6 months.** | **Tecniplast** - Clean Biofilter- Chg UV Lamps- Clean System**Annual Service** |
| **January** |  |  |  |  |  |  |  |
| **February** |  |  |  |  |  |  |  |
| **March** | \*calibrate |  |  |  |  |  |  |
| **April** |  |  |  |  |  |  |  |
| **May** |  |  |  |  |  |  |  |
| **June** | \*calibrate |  |  |  |  |  |  |
| **July** |  |  |  |  |  |  |  |
| **August** |  |  |  |  |  |  |  |
| **September** | \*calibrate |  |  |  |  |  |  |
| **October** |  |  |  |  |  |  |  |
| **November** |  |  |  |  |  |  |  |
| **December** | \*calibrate |  |  |  |  |  |  |

CMDC #274

Effective 2/21